Lab 1 Notes

Packet Sniffer has two parts

1. packet capture library
   1. receives a copy of every link-layer frame that is sent from or received by the computer
2. Packet analyzer
   1. displays the contents of all fields within the protocol message

Once an interface is selected you will get:

* Command Menus
* Packet Display Filter Field
* Packet Listing Window
* Packet Header details window
* Packet contents window in ASCII and hexadecimal